ST700 Series Premium Industrial Vinyl
Application:	General industrial labels
Outside durability    Average 7 to 10 years 
Adhesive:	Permanent Acrylic
Application Temp:	Between 10° and 28° degrees
Users Temp.:          Between -40° and 80° degrees	

HT700 Series High Tack Vinyl
Application:	For difficult surfaces, low energy plastic, lightly oiled surfaces, concrete, 
                                and wood 
Outside durability:   Average 7 to 10 years
Adhesive:                High Strength, Permanent Acrylic
Application Temp:   Between 10° and 28° degrees
Users Temp:           Between  -40° and 80° degrees	
	
E300 Series Standard Vinyl
Application:	Warehouse and general industrial labels
Outside durability: 	Between 3 to 5 years 
Adhesive:	Permanent Acrylic
Application Temp:	Between 10° and 28° degrees
Users Temp:           Between -40° and 80° degrees	

PT700 Series Industrial Polyester
Application:	    For machine plates and non-vinyl applicable surfaces e.g.: Inox/stainless steel
Outside durability: 	Meets UL approved outdoor conditions
Adhesive:	High Strength, Permanent Acrylic
Application Temp:	Between 10° and 28°  degrees
Users Temp:	Between  -40° and 120° degrees	

Specifications of other special tape materials available on request

Important
The values and data on applications and indications and durability are based on tests we believe to be reliable, but which we are under no warranty obligations arising there from.

ST700 Series Premium Vinyl
For all industrial label applications,  5 to 7 years outside	
Tape Width x 30m	150mm	220mm	
			
Clear	ST10130150	ST10130220	
White	ST11030150	ST11030220	
Yellow	ST12030150	ST12030220	
Orange	ST13030150	ST13030220	
Pink	ST13330150	ST13330220	
Red	ST13530150	ST13530220	
Dark Green Sign	ST14030150	ST14030220	
Light Green pipe marker	ST14530150	ST14530220	
Dark Blue sign	ST15030150	ST15030220	
Light Blue pipe marker	ST15530150	ST15530220	
Brown pipe marker	ST16030150	ST16030220	
Dark Brown	ST16330150	ST16330220	
Ligth Brown 	ST16530150	ST16530220	
Purple pipe marker	ST17030150	ST17030220	
Silver Grey pipe marker	ST17530150	ST17530220	
Black	ST18030150	ST18030220	

HT700 Series High Tack Vinyl
For difficult surfaces, low energy plastic, lightly oiled surfaces, concrete, and wood. Fully conformable to shaped and molded surfaces 5 to 7 years outside durability (High Tack Adhesive)	
Tape Width x 30m	150mm	220mm	
Price per roll     			
Clear	ST10130150	ST10130220	
White	ST11030150	ST11030220	
Yellow	ST12030150	ST12030220	
Orange	ST13030150	ST13030220	
Pink	ST13330150	ST13330220	
Red	ST13530150	ST13530220	
Dark Green sign 	ST14030150	ST14030220	
Light Green pipe marker	ST14530150	ST14530220	
Dark Blue sign	ST15030150	ST15030220	
Light Blue pipe marker	ST15530150	ST15530220	
Brown pipe marker	ST16030150	ST16030220	
Dark Brown	ST16330150	ST16330220	
Light Brown	ST16530150	ST16530220	
Purple pipe marker	ST17030150	ST17030220	
Silver Grey pipe marker	ST17530150	ST17530220	
Black	ST18030150	ST18030220	

E300 Series Standard Vinyl
High quality vinyl, indoors and outdoors
3-5  years outdoor durability	
Tape Width x 30m	150mm	220mm	
			
White	ST31030150	ST31030220	
Yellow	ST32030150	ST32030220	

PT700 Industrial Polyester
For machine plates and non-vinyl applicable surfaces e.g. stainless steel	
Tape Width x 30m	150mm	220mm	
			
Mat Alum.	ST22330150	ST22330220	
Gloss White	ST21130150	ST21130220	

PT700 Industrial Polyester
For machine plates and non-vinyl applicable surfaces e. stainless steel	
Tape Width x 20m	150mm	220mm	
			
Glossy Alum. High Tack Adhesive	ST22420150	ST22420220	

H250 High Temperature Vinyl
For use in temperatures up to 250° degrees	
Tape Width x 20m	150mm	220mm	
			
White	ST81020150	ST81020220	

CW200 Cold Weather Vinyl 
For use in temperatures as low as  – 25° degrees	
Tape Width x 24m	150mm	220mm	
	R4144.00	R5929.00	
Yellow	ST12524150	ST12524220	

ReGLO Photoluminescent Vinyl
Meets DIN – IMO – EMED – PSPA Class C requirements	
Tape Width x 15m	150mm	220mm	
			
ReGLO Photolum	ST41015150	ST41015220	

FT500 High Fluorescent tape
High quality caste vinyl. Long term indoor use – outdoor max. 2 years	
Tape Width x 25m	150mm	220mm	
			
Yellow	ST62025150	ST62025220	
Orange/Red	ST63025150	ST63025220	
Pink	ST63325150	ST63325220	
Green	ST64025150	ST64025220	

SR10 Industrial Resin print ribbon
	
Ribbon Width x 120m	230mm	
		
Black	SR10-951230	
White	SR10-955230	
Red	SR10-965230	
Green	SR10-975230	
Blue Sign	SR10-980230	
Yellow	SR10-990230	

Die-Cut Labels. White.

E300 Series Standard Vinyl
3-5 years outdoor durability
Example	Label Width x Length
Total ± 50 m on a roll	148mm x 105mm (A6 – 450 pcs)	210mm x 148mm       (A5 -333 pcs)	210mm x 297mm     
 (A4 – 167 pcs.)	
					
	White	E15310148105	E15310210148	E15310210297	

Preprinted die-cut labels, for one colour overprinting.

Example	Art. number	Description	Colour	210mm x 297mm     
 (A4 – 167 pcs.)	
	E15310210297120	Warning	Yellow on White		

Example	Art. number	Description	Colour	210mm x 297mm     
 (A4 – 167 pcs.)	
	E15310210297150	Mandatory	Blue on White		

Example	Art. number	Description	Colour	210mm x 297mm     
 (A4 – 167 pcs.)	
	E15310210297135	Prohibition	Red on White		
	E15310210297136	Fire Information	Red on White		
	E15310210297140	Safe Condition	Green on White